ELO Touch driver v3.2
Release date: 06-16-2006

Description:
------------
Install.bat - Install to local disk

B46inst.BAT - setting the ELO Touch driver on B45/B46 motherboard.
B55.BAT     - setting the ELO Touch driver on B55 motherboard.
B75.BAT     - setting the ELO Touch driver on B75 motherboard.
B76.BAT     - setting the ELO Touch driver on B76 motherboard.
B77.BAT     - setting the ELO Touch driver on B77 motherboard.
B81.BAT     - setting the ELO Touch driver on B81 motherboard.
B82.BAT     - setting the ELO Touch driver on B82 motherboard.
NM9835.BAT  - setting the ELO Touch driver that use the NetMos Nm9835 PCI serial port.
F81216D.BAT - setting the ELO Touch driver that use the Fintek F81216D serial port.
