Driver and file downloads - Elo TouchSystems - Tyco Electronics

## [Web site]

Linux

The Linux Package Manager has been replaced with the Linux pre-built drivers section, where you can download pre-built driver packages for selected Linux distributions. If you do not see the specific configuration you need on that page, download the serial or USB unified driver (below) to compile your own driver package. Contact Elo for special requests.
Corporate clients: Elo has developed Linux drivers for specific companies.

Download | Version | OS | Interface | Technology | Notes
--- | --- | --- | --- | --- | ---
Linux pre-built drivers | N/A | Linux Kernel 2.4 - 2.6 | USB | IntelliTouch, AccuTouch, CarrollTouch, Surface Capacitive | Pre-built binaries for popular Linux distributions.
Unified_USB_Driver_v3.1.tar.gz (140K) | 3.1 | Linux Kernel 2.6.24 and lower; GCC version 3.3.5 or later; Not compatible with Xserver 1.5 RC or later | USB | IntelliTouch, AccuTouch, CarrollTouch, Surface Capacitive | Manual installer for recent distributions not supported in the Linux pre-built drivers section. Driver supports single monitor, single touchscreen and video rotation. New features. Installation instructions.
Unified_Serial_Driver_v3.1.tar.gz (131K) | 3.1 | Linux Kernel 2.4 - 2.6; not compatible with Xserver 1.4 or later | Serial | IntelliTouch, AccuTouch, CarrollTouch, Surface Capacitive | Manual installer for serial driver with support for multiple monitors, multiple touchscreens and precalibration. New features. Installation instructions.